{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":111,"n_cols":11,"rows_kept":111,"cut":false,"hidden":false,"merged":[[93,5,94,5],[93,6,94,6],[0,0,1,10],[104,1,104,3],[105,2,105,3],[105,8,105,9],[107,2,107,3],[93,0,94,0],[93,1,94,1],[93,2,94,2],[93,3,94,3],[93,4,94,4]],"flags":["formulas_cached_only"]}
[" Analog Bill Of Materials for GAS DETECTOR DEMO - EVAL-CN0234-SDPZ Rev2.pcb on 23/3/2012 "]
[]
["Name","Part Description","Value","Tolerance","PCB Decal","SMD","Layer Name","PART DESC","MFG #1","Part Number","STOCK CODE"]
["B1","BATT-AAA-X1-SMT-CLIPSX2",null,null,"BATT-AAA-X1-SMT-CLIPSX2","Yes","Top","CLIP (x2) BATTERY AAA/N SMT","KEYSTONE","55TR (x2)","Digikey 55KCT-ND (x2)"]
["B2","BATT-AAA-X1-SMT-CLIPSX2",null,null,"BATT-AAA-X1-SMT-CLIPSX2","Yes","Top","CLIP (x2) BATTERY AAA/N SMT","KEYSTONE","55TR (x2)","Digikey 55KCT-ND (x2)"]
["C1","CAP0603","0.1uF",0.1,"C0603","Yes","Top","CAP,SM,0.1UF,25V,X7R,0603,10%","Murata","GRM188R71E104KA01D","Digikey 490-1524-2-ND"]
["C2","CAP0603","DNP",0.1,1206,"Yes","Top","CAP,SM,10UF,6.3V,X5R,1206,10%","TDK","C3216X5R0J106K/1.60","Do Not Place"]
["C3","CAP0603","0.1uF",0.1,"C0603","Yes","Bottom","CAP,SM,0.1UF,25V,X7R,0603,10%","Murata","GRM188R71E104KA01D","Digikey 490-1524-2-ND"]
["C4","CAP0603","0.1uF",0.1,"C0603","Yes","Top","CAP,SM,0.1UF,25V,X7R,0603,10%","Murata","GRM188R71E104KA01D","Digikey 490-1524-2-ND"]
["C5","CAP0603","DNP",0.1,"C0603","Yes","Top","CAP,SM,0.1UF,25V,X7R,0603,10%","Murata","GRM188R71E104KA01D","Do Not Place"]
["C6","CAP0603","DNP",0.1,"C0603","Yes","Top","CAP,SM,0.1UF,25V,X7R,0603,10%","Murata","GRM188R71E104KA01D","Do Not Place"]
["C7","CAP0603","0.1uF",0.1,"C0603","Yes","Top","CAP,SM,0.1UF,25V,X7R,0603,10%","Murata","GRM188R71E104KA01D","Digikey 490-1524-2-ND"]
["C8","CAP0603","0.1uF",0.1,"C0603","Yes","Top","CAP,SM,0.1UF,25V,X7R,0603,10%","Murata","GRM188R71E104KA01D","Digikey 490-1524-2-ND"]
["C9","CAP0603","DNP",0.05,1206,"Yes","Top","CAP,SM,0.02UF,50V,C0G,1206,5%","Murata","GRM3195C1H203JA01D","Do Not Place"]
["C10","CAP0603","DNP",0.1,"C0603","Yes","Top","CAP,SM,0.1UF,25V,X7R,0603,10%","Murata","GRM188R71E104KA01D","Do Not Place"]
["C11","CAP0603","DNP",0.1,"C0603","Yes","Top","CAP,SM,0.1UF,25V,X7R,0603,10%","Murata","GRM188R71E104KA01D","Do Not Place"]
["C12","CAP0603","DNP",0.05,1206,"Yes","Top","CAP,SM,0.02UF,50V,C0G,1206,5%","Murata","GRM3195C1H203JA01D","Do Not Place"]
["C13","CAP0603","0.02uF",0.05,1206,"Yes","Bottom","CAP,SM,0.02UF,50V,C0G,1206,5%","Murata","GRM3195C1H203JA01D","Digikey 490-1760-1-ND"]
["C14","CAP0603","DNP",0.1,"C0603","Yes","Top","CAP,SM,0.1UF,25V,X7R,0603,10%","Murata","GRM188R71E104KA01D","Do Not Place"]
["C15","CAP0603","DNP",0.05,1206,"Yes","Bottom","CAP,SM,0.02UF,50V,C0G,1206,5%","Murata","GRM3195C1H203JA01D","Do Not Place"]
["C16","CAP1210","22uF",0.2,1210,"Yes","Bottom","CAP,SM,22UF,25V,X5R,20%","Taiyo Yuden","TMK325BJ226MM-T","Digikey 587-2086-1-ND"]
["C17","CAP1210","22uF",0.2,1210,"Yes","Bottom","CAP,SM,22UF,25V,X5R,20%","Taiyo Yuden","TMK325BJ226MM-T","Digikey 587-2086-1-ND"]
["C18","CAP1210","22uF",0.2,1210,"Yes","Bottom","CAP,SM,22UF,25V,X5R,20%","Taiyo Yuden","TMK325BJ226MM-T","Digikey 587-2086-1-ND"]
["C19","CAP0603","0.1uF",0.1,"C0603","Yes","Top","CAP,SM,0.1UF,25V,X7R,0603,10%","Murata","GRM188R71E104KA01D","Digikey 490-1524-2-ND"]
["C20","CAP0603","10uF",0.1,1206,"Yes","Bottom","CAP,SM,10UF,6.3V,X5R,1206,10%","TDK","C3216X5R0J106K/1.60","Digikey 445-1388-1-ND"]
["C21","CAP0603","0.02uF",0.05,1206,"Yes","Bottom","CAP,SM,0.02UF,50V,C0G,1206,5%","Murata","GRM3195C1H203JA01D","Digikey 490-1760-1-ND"]
["C22","CAP0603","0.02uF",0.05,1206,"Yes","Bottom","CAP,SM,0.02UF,50V,C0G,1206,5%","Murata","GRM3195C1H203JA01D","Digikey 490-1760-1-ND"]
["C23","CAP1206","2.2uF",0.1,1206,"Yes","Top","CAP,SM,2.2UF,16V,10%,X7R","Murata","GRM31MR71C225KA35L","Digikey 490-1799-1-ND"]
["C24","CAP0603","0.1uF",0.1,"C0603","Yes","Bottom","CAP,SM,0.1UF,25V,X7R,0603,10%","Murata","GRM188R71E104KA01D","Digikey 490-1524-2-ND"]
["C25","CAP1206","2.2uF",0.1,1206,"Yes","Top","CAP,SM,2.2UF,16V,10%,X7R","Murata","GRM31MR71C225KA35L","Digikey 490-1799-1-ND"]
["C26","CAP0603","DNP",0.1,"C0603","Yes","Bottom","CAP,SM,0.1UF,25V,X7R,0603,10%","Murata","GRM188R71E104KA01D","Do Not Place"]
["C27","CAP0603","DNP",0.05,1206,"Yes","Top","CAP,SM,0.02UF,50V,C0G,1206,5%","Murata","GRM3195C1H203JA01D","Do Not Place"]
["C28","CAP0603","0.1uF",0.1,"C0603","Yes","Bottom","CAP,SM,0.1UF,25V,X7R,0603,10%","Murata","GRM188R71E104KA01D","Digikey 490-1524-2-ND"]
["C29","CAP0603","0.1uF",0.1,"C0603","Yes","Bottom","CAP,SM,0.1UF,25V,X7R,0603,10%","Murata","GRM188R71E104KA01D","Digikey 490-1524-2-ND"]
["C30","CAP0603","DNP",0.05,1206,"Yes","Bottom","CAP,SM,0.02UF,50V,C0G,1206,5%","Murata","GRM3195C1H203JA01D","Do Not Place"]
["C31","CAP0603","0.1uF",0.1,"C0603","Yes","Bottom","CAP,SM,0.1UF,25V,X7R,0603,10%","Murata","GRM188R71E104KA01D","Digikey 490-1524-2-ND"]
["J1","CON-SIP-2P","DNP",null,"SIP-2P","No","Top","2 Pin (2x1) Header, 2.54mm Pitch, 1.0mm hole","Harwin","M20-9990246","Do Not Place"]
["J2","TERMINAL_BLOCK_(3.5MM)_2WAY",null,null,"TERMINAL_BLOCK_(3.5MM)2WAY","No","Top","TERMINAL BLOCK, 3.5MM, 2WAY","WIELAND ELECTRIC","25.195.0253.0","FEC 1142156"]
["J3","JUMPER2\\0603_BRIDGE",null,null,"0603-3PIN_BRIDGE","Yes","Bottom","2-Way Shorting Option - Use 0r 0603 Resistor in Position \"A\"","Multicomp","ERJ-3GEY0R00V","Digikey P0.0GTR-ND"]
["J4","CON-RCPT-19P-SAMTEC-SSW-119-02-T-S",null,null,"HEADER19_SIL","No","Top","CONN RCPT .100\" 19POS SNGL TIN","SAMTEC","SSW-119-02-T-S","Digikey SAM1222-19-ND"]
["J5","CON-RCPT-24P-SAMTEC-SSW-124-02-T-S",null,null,"HEADER24_SIL","No","Top","CONN RCPT .100\" 24POS SNGL TIN","SAMTEC","SSW-124-02-T-S","Digikey SAM1222-24-ND"]
["J6","BERG2-10",null,null,"BERG2-10","Yes","Bottom","CONN,SM,10 POS MALE HADER, 0.1IN","FCI","95278-101A10LF","Digikey 609-3483-1-ND"]
["L1","IND","1K@100MHz",null,603,"Yes","Bottom","IND,SM,0603,FERRITE 330Ohms@100MHz","Murata","BLM18AG331SN1D","Digikey 490-5245-1-ND"]
["L2","IND","1.5uH",0.3,1210,"Yes","Bottom","IND,SM,1210, 1.5UH, 1.8A SAT","Taiyo Yuden","NR3015T1R5N","Digikey 587-2617-1-ND"]
["LED1","LED","YELLOW",null,"LED","No","Top","LED,SM,3MM,2mA,YELLOW","KingBright Corp","WP7104LYD","Digikey 754-1247-ND"]
["Q1","MMBFJ177",null,null,"SOT23-3","Yes","Top","TRANSISTOR,SM, MMBFJ177 P-CHAN JFET, SOT23","FAIRCHILD","MMBFJ177","Digikey MMBFJ177CT-ND"]
["Q2","NTR2101PT1GOSCT",null,null,"SOT23","Yes","Bottom","TRANSISTOR,SM,P-FET,NTR2101P, 8V MAX","Infineon","NTR2101PT1GOSCT","Digkey NTR2101PT1GOSCT-ND"]
["R1","RES0603","1K",0.005,"R0603","Yes","Top","RES,SM,THINFILM,1K,1/10W,0.5%,0603","Yageo","RT0603DRD071KL","Digikey 311-1.0KDCT-ND"]
["R2","RES0603","1K",0.005,"R0603","Yes","Top","RES,SM,THINFILM,1K,1/10W,0.5%,0603","Yageo","RT0603DRD071KL","Digikey 311-1.0KDCT-ND"]
["R3","RES0603",0,0,"R0603","Yes","Top","RES,SM,0 OHMS,0603","Panasonic","ERJ-3GEY0R00V","Digikey P0.0GTR-ND"]
["R4","RES0603","11K",0.005,"R0603","Yes","Top","RES,SM,THINFILM,11K,1/10W,0.5%,0603","Yageo","RT0603DRD0711KL","Digikey 311-11KDCT-ND"]
["R5","RES_0R","DNP",0.005,"R0603","Yes","Top","RES,SM,0603,100K,1%,1/10W,0.5%","Yageo","RT0603DRD07100KL","Do Not Place"]
["R6","RES0603","DNP",0.005,"R0603","Yes","Top","RES,SM,THINFILM,12.4K,1/10W,0.5%,0603","Yageo","RT0603DRD0712K4L","Do Not Place"]
["R7","RES0603","DNP",0.01,"R0603","Yes","Top","RES,SM,THINFILM,33,1/10W,1%,0603","Vishay","MCT06030C3309FP500","Do Not Place"]
["R8","RES0603",0,0,"R0603","Yes","Top","RES,SM,0 OHMS,0603","Panasonic","ERJ-3GEY0R00V","Digikey P0.0GTR-ND"]
["R9","RES0603",0,0,"R0603","Yes","Bottom","RES,SM,0 OHMS,0603","Panasonic","ERJ-3GEY0R00V","Digikey P0.0GTR-ND"]
["R10","RES0603","DNP",0.005,"R0603","Yes","Top","RES,SM,THINFILM,12.4K,1/10W,0.5%,0603","Yageo","RT0603DRD0712K4L","Do Not Place"]
["R11","RES0603","DNP",0.005,"R0603","Yes","Top","RES,SM,THINFILM,12.4K,1/10W,0.5%,0603","Yageo","RT0603DRD0712K4L","Do Not Place"]
["R12","RES0603","1MEG",0.01,"R0603","Yes","Top","RES,SM,THICKFILM,1MEG,1/10W,1%,0603","Panasonic","ERJ-3EKF1004V","Digikey P1.00MHTR-ND"]
["R13","RES0603","330K",0.005,"R0603","Yes","Bottom","RES,SM,THINFILM,330K,1/10W,0.5%,0603","Yageo","RT0603DRD07330KL","Digikey 311-330KDCT-ND"]
["R14","RES0603","DNP",0.005,"R0603","Yes","Bottom","RES,SM,THINFILM,11K,1/10W,0.5%,0603","Yageo","RT0603DRD0711KL","Do Not Place"]
["R15","RES0603","DNP",0.005,"R0603","Yes","Bottom","RES,SM,THINFILM,1K,1/10W,0.5%,0603","Yageo","RT0603DRD071KL","Do Not Place"]
["R16","RES0603","DNP",0.005,"R0603","Yes","Bottom","RES,SM,THINFILM,47K,1/10W,0.5%,0603","Yageo","RT0603DRD0747KL","Do Not Place"]
["R17","RES_0R","DNP",null,"R0603","Yes","Bottom","n/a","n/a","n/a","Do Not Place"]
["R18","RES_0R","100K",0.005,"R0603","Yes","Bottom","RES,SM,0603,100K,1%,1/10W,0.5%","Yageo","RT0603DRD07100KL","Digikey 311-100KDCT-ND"]
["R19","RES_0R","100K",0.005,"R0603","Yes","Bottom","RES,SM,0603,100K,1%,1/10W,0.5%","Yageo","RT0603DRD07100KL","Digikey 311-100KDCT-ND"]
["R20","RES0603","36.5K",0.005,"R0603","Yes","Bottom","RES,SM,THINFILM,36.5K,1/16W,0.5%,0603","Susumu","RR0816P-3652-D-55C","Digikey RR08P36.5KDCT-ND"]
["R21","RES0603","12.4K",0.005,"R0603","Yes","Bottom","RES,SM,THINFILM,12.4K,1/10W,0.5%,0603","Yageo","RT0603DRD0712K4L","Digikey 311-12.4KDCT-ND"]
["R22","RES0603","12.4K",0.005,"R0603","Yes","Bottom","RES,SM,THINFILM,12.4K,1/10W,0.5%,0603","Yageo","RT0603DRD0712K4L","Digikey 311-12.4KDCT-ND"]
["R23","RES0603",33,0.01,"R0603","Yes","Bottom","RES,SM,THINFILM,33,1/10W,1%,0603","Vishay","MCT06030C3309FP500","Digikey MCT0603-33.0-CFCT-ND"]
["R24","RES0603","11.5k",0.005,"R0603","Yes","Bottom","RES,SM,THINFILM,11.5K,1/10W,0.5%,0603","Yageo","RT0603DRD0711K5L","Digikey 311-11.5KDCT-ND"]
["R25","RES_0R","100K",0.005,"R0603","Yes","Bottom","RES,SM,0603,100K,1%,1/10W,0.5%","Yageo","RT0603DRD07100KL","Digikey 311-100KDCT-ND"]
["R26","RES0603",330,0.005,"R0603","Yes","Top","RES,SM,330,THINFILM,0.5%","Yageo","RT0603DRD07330RL","Digikey 311-330DCT-ND"]
["R27","VRES-TOP-ADJ","DNP",null,"VRES-TOP-ADJ","No","Top","50k External pot","n/a","n/a","Do Not Place"]
["R28","RES0603",0,0,"R0603","Yes","Bottom","RES,SM,0 OHMS,0603","Panasonic","ERJ-3GEY0R00V","Digikey P0.0GTR-ND"]
["R29","RES0603",0,0,"R0603","Yes","Bottom","RES,SM,0 OHMS,0603","Panasonic","ERJ-3GEY0R00V","Digikey P0.0GTR-ND"]
["R30","THERMISTOR","DNP",0.05,805,"Yes","Top","THERMISTOR, NTC SMD","VISHAY BC COMPONENTS","238161513103 - 10kOhms","Do Not Place"]
["R31","RES-1/8W","DNP",null,"R1/8WA","No","Top","THERMISTOR,TH,NTC, 10K@25C","Murata","NTSD1XH103FPB30","Do Not Place"]
["R32","RES0603","DNP",0.005,"R0603","Yes","Bottom","RES,SM,THINFILM,330K,1/10W,0.5%,0603","Yageo","RT0603DRD07330KL","Do Not Place"]
["R33","RES0603",0,0,"R0603","Yes","Bottom","RES,SM,0 OHMS,0603","Panasonic","ERJ-3GEY0R00V","Digikey P0.0GTR-ND"]
["R34","RES0603",0,0,"R0603","Yes","Bottom","RES,SM,0 OHMS,0603","Panasonic","ERJ-3GEY0R00V","Digikey P0.0GTR-ND"]
["R35","RES0603",0,0,"R0603","Yes","Bottom","RES,SM,0 OHMS,0603","Panasonic","ERJ-3GEY0R00V","Digikey P0.0GTR-ND"]
["R36","RES0603",0,0,"R0603","Yes","Bottom","RES,SM,0 OHMS,0603","Panasonic","ERJ-3GEY0R00V","Digikey P0.0GTR-ND"]
["R37","RES0603","1K",0.005,"R0603","Yes","Bottom","RES,SM,THINFILM,1K,1/10W,0.5%,0603","Yageo","RT0603DRD071KL","Digikey 311-1.0KDCT-ND"]
["R38","RES_0R","100K",0.005,"R0603","Yes","Bottom","RES,SM,0603,100K,1%,1/10W,0.5%","Yageo","RT0603DRD07100KL","Digikey 311-100KDCT-ND"]
["R39","RES0603",0,0,"R0603","Yes","Bottom","RES,SM,0 OHMS,0603","Panasonic","ERJ-3GEY0R00V","Digikey P0.0GTR-ND"]
["R40","RES0603",0,0,"R0603","Yes","Bottom","RES,SM,0 OHMS,0603","Panasonic","ERJ-3GEY0R00V","Digikey P0.0GTR-ND"]
["R41","RES0603",0,0,"R0603","Yes","Bottom","RES,SM,0 OHMS,0603","Yageo","RT0603DRD071KL","Digikey P0.0GTR-ND"]
["SW1","SW-SLIDE-RA-SPDT-ALPS-SSSS916400",null,null,"SW-SLIDE-RA-SPDT","No","Top","SLIDE SWITCH, SPDT, HORIZ","ALPS","SSSS916400","FEC 1123880"]
["U1","ADR3425ARJZ","DNP",null,"SOT23-6","Yes","Top","IC,SM,2.5V PRECISION REFERENCE","Analog Devices","ADR3425ARJZ-R2","Do Not Place"]
["U2","ADA4528-1ARMZ","DNP",null,"MSO8","Yes","Top","IC,SM,AD8675 ZERO DRIFT OPAMP","Analog Devices","ADA4528-1ARMZ","Do Not Place"]
["U3","ADR291GRZ",null,null,"SO8NB","Yes","Top","Low Noise Micropower Precision Voltage Reference (2.5 V),SOIC-8","Analog Devices","ADR291GRZ","ADR291GRZ"]
["U4","ADCMP370AKS","DNP",null,"SC70-5","Yes","Bottom","IC,SM,ADCMP370 LOW POWER COMPARATOR","Analog Devices","ADCMP370AKSZ","Do Not Place"]
["U5","CO-AX",null,null,"CO-AX_SENSOR","No","Top","CONN RECEPT PIN .048-.064\" .100\" (Solder into PCB)","Mill-Max","0364-0-15-15-13-27-10-0","3x Digikey ED90089-ND"]
[{"$nulls":7},"SENSOR,TH,CARBON MONOXIDE (Fit into Recept Pins)","Alphasense","CO-AX","Buy direct from Alphasense PN: CO-AX"]
["U6","ADP2503ACPZ",null,null,"LFCSP-10-3MM","Yes","Bottom","DC/DC Converter","Analog Devices","ADP2503ACPZ","ADP2503ACPZ"]
["U7","AD7798/99",null,null,"TSSOP-16","Yes","Top","IC,SM,AD7798,Lo-Popwer 16/24 Bit Sigma Delta ADC","Analog Devices","AD7798/AD7798BRU","AD7798BRUZ"]
["U8","ADA4528-1ARMZ","DNP",null,"MSO8","Yes","Top","IC,SM,AD8675 ZERO DRIFT OPAMP","Analog Devices","ADA4528-1ARMZ","Do Not Place"]
["U9","AD8500","DNP",null,"SC70-5","Yes","Top","Micropower Precision CMOS Operational Amplifier","Analog Devices","AD8500AKSZ","Do Not Place"]
["U10","ADA4505-2ARMZ",null,null,"MSO8","Yes","Bottom","IC,SM,MICROPOWER OPAMP, MSOP8","Analog Devices","ADA4505-2ARMZ","ADA4505-2ARMZ"]
["U11","AD8500AKSZ",null,null,"SC70-5","Yes","Bottom","Micropower Precision CMOS Operational Amplifier","Analog Devices","AD8500AKSZ","Do Not Place"]
["U13","24LC64","24LC64",null,"SO8NB","Yes","Bottom","64K I2C Serial EEPROM","Microchip Technology","24LC64-ISN","FEC 975-8070"]
[]
[]
[null,"Distributor Web Sites"]
[null,"FEC","www.farnell.com",{"$nulls":4},"PCB","GAS DETECTOR DEMO - EVAL-CN0234-SDPZ Rev2",null,"n/a"]
[null,"Digikey","www.digikey.com",{"$nulls":4},"Anti-Static Bag"]
[null,"Analog Devices","www.analog.com",{"$nulls":4},"Bar Code Box Label","Part No: EVAL-CN0234-SDPZ\nDescription: GAS DETECTOR DEMO KIT",null,"ADI Supplied"]
[{"$nulls":7},"Small White Eval Box"]
[{"$nulls":7},"Anti-Static Bubble Wrap"]
[{"$nulls":7},"Gas Detector to SDP Adapter Board","Analog Devices","Gas Detector to SDP Adapter Board","Gas Detector to SDP Adapter Board"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}